|  |  |
| --- | --- |
|  |  |
|  |  |
|  |  |
|  | Review  Minutes of Meeting  TSP Release Layout |
|  | Work Product for review:  Date: 2020-04-06 |

# Scope of Work

These are the minutes from the review regarding TCP release Schematic.

The matters appeared during the review will be treated by the author or by the responsible person, and you will later be informed about the conclusion of the matters.

Should you have comments on any of the following points please involve the Review leader of this review meeting no later that 2 days after the Meeting of Minutes have been puplished to the team.

# Meeting Result

|  |  |
| --- | --- |
| Participants | SKHO,BGS,KAMA,AMN |
| Review leader/ moderator | SKHO |
| Author | SKHO |
| Project name | [Project name or title] |
| Scope of review | Review of TSP release Schematic |
| Date, time | 22/04-2020 |

|  |  |  |
| --- | --- | --- |
| **Conclusion** | **Status** | **Comments** |
| The review was approved by all participants? | Yes | Approved with corrections |
| Are there any RISK? | No |  |
| Do all findings have a responsible person? | Yes |  |
| Is there a deadline on all findings? | Yes |  |
| Any other matters? | No |  |

# Findings

|  |  |  |  |
| --- | --- | --- | --- |
| **Action** | **Comment** | **Responsible** | **Deadline** |
| Jakob: alle holes Ø2.2 | Done | SKHO | [dmy] |
| Larger Cut out under Burn Resister | Done | SKHO | [dmy] |
|  |  |  |  |
| 1. Mangler teardrops 2. ~20x8 mm Her kunne man nok nøjes med én via og så route begge dertil   cid:image001.png@01D61CAA.C9BF3DE0   1. 25x7 mm Kan placeres I pad   cid:image012.png@01D61CAA.C9BF3DE0 | DONE |  |  |
|  |  |  |  |
| 1. Hvorfor de polygon cutouts? | To keep the heat in onlt the burn resiser |  |  |
| 1. Havde været nemmere med en ”region”   cid:image013.png@01D61CA9.C194BF10 | Done |  |  |
| 1. 26x9 mm øverste via kan placeres i pad (5) og nederste kan spares, rout op til banen. cid:image014.png@01D61CAA.C9BF3DE0 | Done |  |  |
| 1. 20.5x9.5 mm kan pladseres i padcid:image015.png@01D61CAA.C9BF3DE0 | Done |  |  |
| consider to go for reed path. | Not possibel will breake GND |  |  |
| Overvej at drukne gnd vias – ACB har kommenteret  dette med hensyn til acid traps overfor mig. | Will ask production again , Not implemented |  |  |
| Consider another route for the connection. The GND plane is unconnected. | Done |  |  |
| Måske skulle du fordele nogle GND vias specielt ved kanten. | Not implimnetet |  |  |

# Other comments